,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
8 ft Opening BCE 36'' Nozzle,BCE-1-36,Powered Aire Unheated Insect Control Air Curtain - BCE-1-36 as Specified,37,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,3100,2200,0.95,0,1,0.5,1400,85,60 dBA
8 ft Opening BCE 42'' Nozzle,BCE-1-42,Powered Aire Unheated Insect Control Air Curtain - BCE-1-42 as Specified,43,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2700,2200,0.93,0,1,0.5,1400,90,60 dBA
8 ft Opening BCE 48'' Nozzle,BCE-1-48,Powered Aire Unheated Insect Control Air Curtain - BCE-1-48 as Specified,49,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2400,2200,0.92,0,1,0.5,1400,100,60 dBA
8 ft Opening BCE 60'' Nozzle 1 Motor,BCE-1-60,Powered Aire Unheated Insect Control Air Curtain - BCE-1-60 as Specified,61,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2100,2200,0.91,0,1,0.5,1400,115,60 dBA
8 ft Opening BCE 60'' Nozzle 2 Motor,BCE-2-60,Powered Aire Unheated Insect Control Air Curtain - BCE-2-60 as Specified,61,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2800,3200,0.95,0,2,0.5,1400,140,>60 dBA
8 ft Opening BCE 72'' Nozzle,BCE-2-72,Powered Aire Unheated Insect Control Air Curtain - BCE-2-72 as Specified,73,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,3100,4300,0.95,0,2,0.5,1400,165,>60 dBA
8 ft Opening BCE 84'' Nozzle,BCE-2-84,Powered Aire Unheated Insect Control Air Curtain - BCE-2-84 as Specified,85,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2700,4300,0.93,0,2,0.5,1400,185,>60 dBA
8 ft Opening BCE 96'' Nozzle,BCE-2-96,Powered Aire Unheated Insect Control Air Curtain - BCE-2-96 as Specified,97,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2400,4300,0.92,0,2,0.5,1400,200,>60 dBA
8 ft Opening BCE 108'' Nozzle,BCE-3-108,Powered Aire Unheated Insect Control Air Curtain - BCE-3-108 as Specified,109,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,3100,6500,0.95,0,3,0.5,1400,240,>60 dBA
8 ft Opening BCE 118'' Nozzle,BCE-3-120,Powered Aire Unheated Insect Control Air Curtain - BCE-3-120 as Specified,119,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2700,6500,0.94,0,3,0.5,1400,270,>60 dBA
8 ft Opening BCE 133'' Nozzle,BCE-3-132,Powered Aire Unheated Insect Control Air Curtain - BCE-3-132 as Specified,134,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,2300,6500,0.95,0,3,0.5,1400,280,>60 dBA
8 ft Opening BCE 145'' Nozzle,BCE-4-144,Powered Aire Unheated Insect Control Air Curtain - BCE-4-144 as Specified,146,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,8,3100,8700,0.95,0,4,0.5,1400,330,>60 dBA
10 ft Opening BCT 36'' Nozzle,BCT-1-36,Powered Aire Unheated Insect Control Air Curtain - BCT-1-36 as Specified,37,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3700,2500,0.95,0,1,0.75,1630,90,63 dBA
10 ft Opening BCT 42'' Nozzle,BCT-1-42,Powered Aire Unheated Insect Control Air Curtain - BCT-1-42 as Specified,43,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3200,2500,0.93,0,1,0.75,1630,100,63 dBA
10 ft Opening BCT 48'' Nozzle,BCT-1-48,Powered Aire Unheated Insect Control Air Curtain - BCT-1-48 as Specified,49,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,2800,2600,0.92,0,1,0.75,1630,105,63 dBA
10 ft Opening BCT 60'' Nozzle 1 Motor,BCT-1-60,Powered Aire Unheated Insect Control Air Curtain - BCT-1-60 as Specified,61,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,2200,2500,0.91,0,1,0.75,1630,120,63 dBA
10 ft Opening BCT 60'' Nozzle 2 Motor,BCT-2-60,Powered Aire Unheated Insect Control Air Curtain - BCT-2-60 as Specified,61,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3300,3800,0.95,0,2,0.75,1630,150,>63 dBA
10 ft Opening BCT 72'' Nozzle,BCT-2-72,Powered Aire Unheated Insect Control Air Curtain - BCT-2-72 as Specified,73,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3700,5100,0.95,0,2,0.75,1630,170,>63 dBA
10 ft Opening BCT 84'' Nozzle,BCT-2-84,Powered Aire Unheated Insect Control Air Curtain - BCT-2-84 as Specified,85,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3200,5100,0.93,0,2,0.75,1630,190,>63 dBA
10 ft Opening BCT 96'' Nozzle,BCT-2-96,Powered Aire Unheated Insect Control Air Curtain - BCT-2-96 as Specified,97,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,2800,5100,0.92,0,2,0.75,1630,205,>63 dBA
10 ft Opening BCT 108'' Nozzle,BCT-3-108,Powered Aire Unheated Insect Control Air Curtain - BCT-3-108 as Specified,109,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3700,7600,0.95,0,3,0.75,1630,245,>63 dBA
10 ft Opening BCT 118'' Nozzle,BCT-3-120,Powered Aire Unheated Insect Control Air Curtain - BCT-3-120 as Specified,119,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3200,7600,0.94,0,3,0.75,1630,275,>63 dBA
10 ft Opening BCT 133'' Nozzle,BCT-3-132,Powered Aire Unheated Insect Control Air Curtain - BCT-3-132 as Specified,134,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,2800,7600,0.95,0,3,0.75,1630,290,>63 dBA
10 ft Opening BCT 145'' Nozzle,BCT-4-144,Powered Aire Unheated Insect Control Air Curtain - BCT-4-144 as Specified,146,USDA  ;  FDA  ;  AIB  ;  ETL Indoor/Outdoor  ;  Made in USA,10,3700,10200,0.95,0,4,0.75,1630,340,>63 dBA
