,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,Temperature Rise_Range##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
Unheated 36'' Nozzle,CED-1-36,Powered Aire Unheated Customer Entry Air Curtain - CED-1-36 as Specified,37,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 CFM Low/High Avg,0.95,0,0,0,1,0.5,1075,85,51 dBA
Unheated 42'' Nozzle,CED-1-42,Powered Aire Unheated Customer Entry Air Curtain - CED-1-42 as Specified,43,ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.93,0,0,0,1,0.5,1075,90,51 dBA
Unheated 48'' Nozzle,CED-1-48,Powered Aire Unheated Customer Entry Air Curtain - CED-1-48 as Specified,49,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,0,0,0,1,0.5,1075,100,51 dBA
Unheated 60'' Nozzle 1 Motor,CED-1-60,Powered Aire Unheated Customer Entry Air Curtain - CED-1-60 as Specified,61,ETL  ;  Made in USA,11,800 - 900 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.91,0,0,0,1,0.5,1075,110,51 dBA
Unheated 60'' Nozzle 2 Motor,CED-2-60,Powered Aire Unheated Customer Entry Air Curtain - CED-2-60 as Specified,61,ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,1500 - 1600 CFM Low/High Avg,0.95,0,0,0,2,0.5,1075,140,>51 dBA
Unheated 72'' Nozzle,CED-2-72,Powered Aire Unheated Customer Entry Air Curtain - CED-2-72 as Specified,73,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,0,0,0,2,0.5,1075,160,>51 dBA
Unheated 84'' Nozzle,CED-2-84,Powered Aire Unheated Customer Entry Air Curtain - CED-2-84 as Specified,85,ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1900 - 2100 CFM Low/High Avg,0.93,0,0,0,2,0.5,1075,180,>51 dBA
Unheated 96'' Nozzle,CED-2-96,Powered Aire Unheated Customer Entry Air Curtain - CED-2-96 as Specified,97,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.92,0,0,0,2,0.5,1075,200,>51 dBA
Unheated 108'' Nozzle,CED-3-108,Powered Aire Unheated Customer Entry Air Curtain - CED-3-108 as Specified,109,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,0,0,0,3,0.5,1075,240,>51 dBA
Unheated 120'' Nozzle,CED-3-120,Powered Aire Unheated Customer Entry Air Curtain - CED-3-120 as Specified,119,ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,0,0,0,3,0.5,1075,270,>51 dBA
Unheated 133'' Nozzle,CED-3-132,Powered Aire Unheated Customer Entry Air Curtain - CED-3-132 as Specified,134,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,0,0,0,3,0.5,1075,280,>51 dBA
Unheated 145'' Nozzle,CED-4-144,Powered Aire Unheated Customer Entry Air Curtain - CED-4-144 as Specified,146,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,3900 - 4300 CFM Low/High Avg,0.95,0,0,0,4,0.5,1075,320,>51 dBA
Elec Heated 36'' Nozzle,CED-1-36E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-1-36E as Specified,37,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 CFM Low/High Avg,0.95,0,10000,33 - 29 Low/High,1,0.5,1075,90,51 dBA
Elec Heated 42'' Nozzle,CED-1-42E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-1-42E as Specified,43,ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.93,0,10000,33 - 29 Low/High,1,0.5,1075,95,51 dBA
Elec Heated 48'' Nozzle,CED-1-48E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-1-48E as Specified,49,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,0,10000,33 - 29 Low/High,1,0.5,1075,100,51 dBA
Elec Heated 60'' Nozzle 1 Motor,CED-1-60E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-1-60E as Specified,61,ETL  ;  Made in USA,11,800 - 900 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.91,0,10000,33 - 29 Low/High,1,0.5,1075,115,51 dBA
Elec Heated 60'' Nozzle 2 Motor,CED-2-60E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-2-60E as Specified,61,ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,1500 - 1600 CFM Low/High Avg,0.95,0,15000,33 - 29 Low/High,2,0.5,1075,150,>51 dBA
Elec Heated 72'' Nozzle,CED-2-72E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-2-72E as Specified,73,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,0,20000,33 - 29 Low/High,2,0.5,1075,170,>51 dBA
Elec Heated 84'' Nozzle,CED-2-84E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-2-84E as Specified,85,ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1900 - 2100 CFM Low/High Avg,0.93,0,20000,33 - 29 Low/High,2,0.5,1075,190,>51 dBA
Elec Heated 96'' Nozzle,CED-2-96E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-2-96E as Specified,97,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.92,0,20000,33 - 29 Low/High,2,0.5,1075,210,>51 dBA
Elec Heated 108'' Nozzle,CED-3-108E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-3-108E as Specified,109,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,0,30000,33 - 29 Low/High,3,0.5,1075,245,>51 dBA
Elec Heated 120'' Nozzle,CED-3-120E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-3-120E as Specified,119,ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.95,0,30000,33 - 29 Low/High,3,0.5,1075,270,>51 dBA
Elec Heated 133'' Nozzle,CED-3-132E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-3-132E as Specified,134,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.95,0,30000,33 - 29 Low/High,3,0.5,1075,285,>51 dBA
Elec Heated 145'' Nozzle,CED-4-144E,Powered Aire Electrically Heated Customer Entry Air Curtain - CED-4-144E as Specified,146,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,3900 - 4300 CFM Low/High Avg,0.95,0,40000,33 - 29 Low/High,4,0.5,1075,345,>51 dBA
