,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,HVAC_BTU Input##other##,Temperature Rise_Range##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
HW Heated 36'' Nozzle,CHS-1-36HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-1-36HW as Specified,39,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 CFM Low/High Avg,0.95,45000,43 - 38 Low/High,1,0.5,1075,125,51-53 dBA
HW Heated 48'' Nozzle,CHS-1-48HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-1-48HW as Specified,51,ARI Standard 410  ;  ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,47000,45 - 40 Low/High,1,0.5,1075,135,51-53 dBA
HW Heated 60'' Nozzle,CHS-1-60HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-1-60HW as Specified,63,ARI Standard 410  ;  ETL  ;  Made in USA,11,800 - 900 FPM Low/High Avg,1000 - 1100CFM Low/High Avg,0.91,45000,43 - 38 Low/High,1,0.5,1075,170,51-53 dBA
HW Heated 72'' Nozzle,CHS-2-72HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-2-72HW as Specified,75.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,82000,39 - 35 Low/High,2,0.5,1075,240,>51-53 dBA
HW Heated 84'' Nozzle,CHS-2-84HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-2-84HW as Specified,87.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1900 - 2100 CFM Low/High Avg,0.93,87000,41 - 37 Low/High,2,0.5,1075,270,>51-53 dBA
HW Heated 96'' Nozzle,CHS-2-96HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-2-96HW as Specified,99.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.92,87000,41 - 37 Low/High,2,0.5,1075,295,>51-53 dBA
HW Heated 108'' Nozzle 2 Motor,CHS-2-108HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-2-108HW as Specified,111.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,85000,40 - 36 Low/High,2,0.5,1075,320,>51-53 dBA
HW Heated 108'' Nozzle 3 Motor,CHS-3-108HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-3-108HW as Specified,111.15625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,127000,40 - 36 Low/High,3,0.5,1075,360,>51-53 dBA
HW Heated 120'' Nozzle,CHS-3-120HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-3-120HW as Specified,123.15625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,131000,41 - 37 Low/High,3,0.5,1075,400,>51-53 dBA
HW Heated 132'' Nozzle,CHS-3-132HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-3-132HW as Specified,135.15625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,138000,44 - 39 Low/High,3,0.5,1075,460,>51-53 dBA
HW Heated 144'' Nozzle,CHS-4-144HW,Powered Aire Water Heated Customer Entry Air Curtain - CHS-4-144HW as Specified,147.21875,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,3900 - 4300 CFM Low/High Avg,0.95,174000,41 - 37 Low/High,4,0.5,1075,480,>51-53 dBA
Steam Heated 36'' Nozzle,CHS-1-36ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-1-36ST as Specified,39,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 CFM Low/High Avg,0.95,59000,56 - 50 Low/High,1,0.5,1075,125,51-53 dBA
Steam Heated 48'' Nozzle,CHS-1-48ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-1-48ST as Specified,51,ARI Standard 410  ;  ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,60000,57 - 51 Low/High,1,0.5,1075,135,51-53 dBA
Steam Heated 60'' Nozzle,CHS-1-60ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-1-60ST as Specified,63,ARI Standard 410  ;  ETL  ;  Made in USA,11,800 - 900 FPM Low/High Avg,1000 - 1100CFM Low/High Avg,0.91,60000,57 - 51 Low/High,1,0.5,1075,170,51-53 dBA
Steam Heated 72'' Nozzle,CHS-2-72ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-2-72ST as Specified,75.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,104000,49 - 44 Low/High,2,0.5,1075,240,>51-53 dBA
Steam Heated 84'' Nozzle,CHS-2-84ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-2-84ST as Specified,87.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1900 - 2100 CFM Low/High Avg,0.93,111000,53 - 47 Low/High,2,0.5,1075,270,>51-53 dBA
Steam Heated 96'' Nozzle,CHS-2-96ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-2-96ST as Specified,99.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.92,108000,51 - 46 Low/High,2,0.5,1075,295,>51-53 dBA
Steam Heated 108'' Nozzle 2 Motor,CHS-2-108ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-2-108ST as Specified,111.0625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,104000,49 - 44 Low/High,2,0.5,1075,320,>51-53 dBA
Steam Heated 108'' Nozzle 3 Motor,CHS-3-108ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-3-108ST as Specified,111.15625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,155000,49 - 44 Low/High,3,0.5,1075,360,>51-53 dBA
Steam Heated 120'' Nozzle,CHS-3-120ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-3-120ST as Specified,123.15625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,162000,51 - 46 Low/High,3,0.5,1075,400,>51-53 dBA
Steam Heated 132'' Nozzle,CHS-3-132ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-3-132ST as Specified,135.15625,ARI Standard 410  ;  ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,162000,51 - 46 Low/High,3,0.5,1075,460,>51-53 dBA
Steam Heated 144'' Nozzle,CHS-4-144ST,Powered Aire Steam Heated Customer Entry Air Curtain - CHS-4-144ST as Specified,147.21875,ARI Standard 410  ;  ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,3900 - 4300 CFM Low/High Avg,0.95,107000,49 - 44 Low/High,4,0.5,1075,480,>51-53 dBA
