,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,HVAC_Temperature Rise##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
11 ft Opening Unheated ECC-E 36'' Nozzle,ECC-E-1-36,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-1-36 as Specified,39,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 CFM Low/High Avg,0.95,0,0,0,1,0.5,1075,170,51 - 53 dBA
11 ft Opening Unheated ECC-E 48'' Nozzle,ECC-E-1-48,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-1-48 as Specified,51,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,0,0,0,1,0.5,1075,190,51 - 53 dBA
11 ft Opening Unheated ECC-E 60'' Nozzle,ECC-E-1-60,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-1-60 as Specified,63,ETL  ;  Made in USA,11,800 - 900 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.91,0,0,0,1,0.5,1075,220,51 - 53 dBA
11 ft Opening Unheated ECC-E 72'' Nozzle,ECC-E-2-72,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-2-72 as Specified,75.0625,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,0,0,0,2,0.5,1075,340,>51 - 53 dBA
11 ft Opening Unheated ECC-E 84'' Nozzle,ECC-E-2-84,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-2-84 as Specified,87.0625,ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1900 - 2100 CFM Low/High Avg,0.93,0,0,0,2,0.5,1075,355,>51 - 53 dBA
11 ft Opening Unheated ECC-E 96'' Nozzle,ECC-E-2-96,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-2-96 as Specified,99.0625,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.92,0,0,0,2,0.5,1075,370,>51 - 53 dBA
11 ft Opening Unheated ECC-E 108'' Nozzle 2 Motor,ECC-E-2-108,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-2-108 as Specified,111.0625,ETL  ;  Made in USA,11,900 - 1100 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,0,0,0,2,0.5,1075,395,>51 - 53 dBA
11 ft Opening Unheated ECC-E 108'' Nozzle 3 Motor,ECC-E-3-108,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-3-108 as Specified,111.15625,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,0,0,0,3,0.5,1075,515,>51 - 53 dBA
11 ft Opening Unheated ECC-E 120'' Nozzle,ECC-E-3-120,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-3-120 as Specified,123.15625,ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,0,0,0,3,0.5,1075,530,>51 - 53 dBA
11 ft Opening Unheated ECC-E 132'' Nozzle,ECC-E-3-132,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-3-132 as Specified,135.15625,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,0,0,0,3,0.5,1075,545,>51 - 53 dBA
11 ft Opening Unheated ECC-E 144'' Nozzle,ECC-E-4-144,Powered Aire Unheated Customer Entry Air Curtain - ECC-E-4-144 as Specified,147.21875,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,3900 - 4300 CFM Low/High Avg,0.95,0,0,0,4,0.5,1075,685,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 36'' Nozzle,ECC-E-1-36E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-1-36E as Specified,39,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1000 CFM Low/High Avg,0.95,0,10000,33 - 29 Low/High,1,0.5,1075,175,51 - 53 dBA
11 ft Opening Elec Heated ECC-E 48'' Nozzle,ECC-E-1-48E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-1-48E as Specified,51,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.92,0,10000,33 - 29 Low/High,1,0.5,1075,200,51 - 53 dBA
11 ft Opening Elec Heated ECC-E 60'' Nozzle,ECC-E-1-60E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-1-60E as Specified,63,ETL  ;  Made in USA,11,800 - 900 FPM Low/High Avg,1000 - 1100 CFM Low/High Avg,0.91,0,10000,33 - 29 Low/High,1,0.5,1075,225,51 - 53 dBA
11 ft Opening Elec Heated ECC-E 72'' Nozzle,ECC-E-2-72E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-2-72E as Specified,75.0625,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,0,20000,33 - 29 Low/High,2,0.5,1075,350,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 84'' Nozzle,ECC-E-2-84E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-2-84E as Specified,87.0625,ETL  ;  Made in USA,11,1200 - 1300 FPM Low/High Avg,1900 - 2100 CFM Low/High Avg,0.93,0,20000,33 - 29 Low/High,2,0.5,1075,365,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 96'' Nozzle,ECC-E-2-96E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-2-96E as Specified,99.0625,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.92,0,20000,33 - 29 Low/High,2,0.5,1075,380,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 108'' Nozzle 2 Motor,ECC-E-2-108E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-2-108E as Specified,111.0625,ETL  ;  Made in USA,11,900 - 1100 FPM Low/High Avg,1900 - 2200 CFM Low/High Avg,0.95,0,20000,33 - 29 Low/High,2,0.5,1075,400,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 108'' Nozzle 3 Motor,ECC-E-3-108E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-3-108E as Specified,111.15625,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.92,0,30000,33 - 29 Low/High,3,0.5,1075,520,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 120'' Nozzle,ECC-E-3-120E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-3-120E as Specified,123.15625,ETL  ;  Made in USA,11,1300 - 1400 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,0,30000,33 - 29 Low/High,3,0.5,1075,550,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 132'' Nozzle,ECC-E-3-132E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-3-132E as Specified,135.15625,ETL  ;  Made in USA,11,1100 - 1200 FPM Low/High Avg,2900 - 3200 CFM Low/High Avg,0.95,0,30000,33 - 29 Low/High,3,0.5,1075,560,>51 - 53 dBA
11 ft Opening Elec Heated ECC-E 144'' Nozzle,ECC-E-4-144E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-E-4-144E as Specified,147.21875,ETL  ;  Made in USA,11,1400 - 1600 FPM Low/High Avg,3900 - 4300 CFM Low/High Avg,0.95,0,40000,33 - 29 Low/High,4,0.5,1075,700,>51 - 53 dBA
