,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,HVAC_Temperature Rise##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
14 ft Opening Unheated ECC 36'' Nozzle,ECC-1-36,Powered Aire Unheated Customer Entry Air Curtain - ECC-1-36 as Specified,39,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.95,0,0,0,1,0.75,1630,180,56 - 63 dBA
14 ft Opening Unheated ECC 48'' Nozzle,ECC-1-48,Powered Aire Unheated Customer Entry Air Curtain - ECC-1-48 as Specified,51,ETL  ;  Made in USA,14,1900 - 2800 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.92,0,0,0,1,0.75,1630,195,56 - 63 dBA
14 ft Opening Unheated ECC 60'' Nozzle,ECC-1-60,Powered Aire Unheated Customer Entry Air Curtain - ECC-1-60 as Specified,63,ETL  ;  Made in USA,14,1500 - 2200 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.91,0,0,0,1,0.75,1630,225,56 - 63 dBA
14 ft Opening Unheated ECC 72'' Nozzle,ECC-2-72,Powered Aire Unheated Customer Entry Air Curtain - ECC-2-72 as Specified,75.0625,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,0,0,0,2,0.75,1630,360,>56 - 63 dBA
14 ft Opening Unheated ECC 84'' Nozzle,ECC-2-84,Powered Aire Unheated Customer Entry Air Curtain - ECC-2-84 as Specified,87.0625,ETL  ;  Made in USA,14,2100 - 3200 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.93,0,0,0,2,0.75,1630,370,>56 - 63 dBA
14 ft Opening Unheated ECC 96'' Nozzle,ECC-2-96,Powered Aire Unheated Customer Entry Air Curtain - ECC-2-96 as Specified,99.0625,ETL  ;  Made in USA,14,1900 - 2800 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.92,0,0,0,2,0.75,1630,385,>56 - 63 dBA
14 ft Opening Unheated ECC 108'' Nozzle 2 Motor,ECC-2-108,Powered Aire Unheated Customer Entry Air Curtain - ECC-2-108 as Specified,111.0625,ETL  ;  Made in USA,14,1700 - 2500 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,0,0,0,2,0.75,1630,400,>56 - 63 dBA
14 ft Opening Unheated ECC 108'' Nozzle 3 Motor,ECC-3-108,Powered Aire Unheated Customer Entry Air Curtain - ECC-3-108 as Specified,111.15625,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,0,0,0,3,0.75,1630,540,>56 - 63 dBA
14 ft Opening Unheated ECC 120'' Nozzle,ECC-3-120,Powered Aire Unheated Customer Entry Air Curtain - ECC-3-120 as Specified,123.15625,ETL  ;  Made in USA,14,2100 - 3200 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,0,0,3,0.75,1630,550,>56 - 63 dBA
14 ft Opening Unheated ECC 132'' Nozzle,ECC-3-132,Powered Aire Unheated Customer Entry Air Curtain - ECC-3-132 as Specified,135.15625,ETL  ;  Made in USA,14,1900 - 2800 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,0,0,3,0.75,1630,565,>56 - 63 dBA
14 ft Opening Unheated ECC 144'' Nozzle,ECC-4-144,Powered Aire Unheated Customer Entry Air Curtain - ECC-4-144 as Specified,147.21875,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,6800 - 10200 CFM Low/High Avg,0.95,0,0,0,4,0.75,1630,720,>56 - 63 dBA
14 ft Opening Elec Heated ECC 36'' Nozzle,ECC-1-36E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-1-36E as Specified,39,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.95,0,10000,19 - 13 Low/High,1,0.75,1630,180,56 - 63 dBA
14 ft Opening Elec Heated ECC 48'' Nozzle,ECC-1-48E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-1-48E as Specified,51,ETL  ;  Made in USA,14,1900 - 2800 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.92,0,10000,19 - 13 Low/High,1,0.75,1630,205,56 - 63 dBA
14 ft Opening Elec Heated ECC 60'' Nozzle,ECC-1-60E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-1-60E as Specified,63,ETL  ;  Made in USA,14,1500 - 2200 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.91,0,10000,19 - 13 Low/High,1,0.75,1630,230,56 - 63 dBA
14 ft Opening Elec Heated ECC 72'' Nozzle,ECC-2-72E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-2-72E as Specified,75.0625,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,0,20000,19 - 13 Low/High,2,0.75,1630,365,>56 - 63 dBA
14 ft Opening Elec Heated ECC 84'' Nozzle,ECC-2-84E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-2-84E as Specified,87.0625,ETL  ;  Made in USA,14,2100 - 3200 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.93,0,20000,19 - 13 Low/High,2,0.75,1630,380,>56 - 63 dBA
14 ft Opening Elec Heated ECC 96'' Nozzle,ECC-2-96E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-2-96E as Specified,99.0625,ETL  ;  Made in USA,14,1900 - 2800 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.92,0,20000,19 - 13 Low/High,2,0.75,1630,400,>56 - 63 dBA
14 ft Opening Elec Heated ECC 108'' Nozzle 2 Motor,ECC-2-108E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-2-108E as Specified,111.0625,ETL  ;  Made in USA,14,1700 - 2500 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,0,20000,19 - 13 Low/High,2,0.75,1630,420,>56 - 63 dBA
14 ft Opening Elec Heated ECC 108'' Nozzle 3 Motor,ECC-3-108E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-3-108E as Specified,111.15625,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,0,30000,19 - 13 Low/High,3,0.75,1630,550,>56 - 63 dBA
14 ft Opening Elec Heated ECC 120'' Nozzle,ECC-3-120E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-3-120E as Specified,123.15625,ETL  ;  Made in USA,14,2100 - 3200 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,30000,19 - 13 Low/High,3,0.75,1630,570,>56 - 63 dBA
14 ft Opening Elec Heated ECC 132'' Nozzle,ECC-3-132E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-3-132E as Specified,135.15625,ETL  ;  Made in USA,14,1900 - 2800 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,30000,19 - 13 Low/High,3,0.75,1630,585,>56 - 63 dBA
14 ft Opening Elec Heated ECC 144'' Nozzle,ECC-4-144E,Powered Aire Electrically Heated Customer Entry Air Curtain - ECC-4-144E as Specified,147.21875,ETL  ;  Made in USA,14,2500 - 3700 FPM Low/High Avg,6800 - 10200 CFM Low/High Avg,0.95,0,40000,19 - 13 Low/High,4,0.75,1630,730,>56 - 63 dBA
