,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,Temperature Rise_Range##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
Elec Heated 36'' Nozzle,ECE-1-36E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-1-36E as Specified,37,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.95,0,10000,19 - 13 Low/High,1,0.75,1630,95,56 - 63 dBA
Elec Heated 42'' Nozzle,ECE-1-42E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-1-42E as Specified,43,ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.93,0,10000,19 - 13 Low/High,1,0.75,1630,100,56 - 63 dBA
Elec Heated 48'' Nozzle,ECE-1-48E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-1-48E as Specified,49,ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.92,0,10000,19 - 13 Low/High,1,0.75,1630,110,56 - 63 dBA
Elec Heated 60'' Nozzle 1 Motor,ECE-1-60E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-1-60E as Specified,61,ETL  ;  Made in USA,12,1500 - 2200 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.91,0,10000,19 - 13 Low/High,1,0.75,1630,120,56 - 63 dBA
Elec Heated 60'' Nozzle 2 Motor,ECE-2-60E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-2-60E as Specified,61,ETL  ;  Made in USA,12,2200 - 3300 FPM Low/High Avg,2600 - 3800 CFM Low/High Avg,0.94,0,15000,19 - 13 Low/High,2,0.75,1630,155,>56 - 63 dBA
Elec Heated 72'' Nozzle,ECE-2-72E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-2-72E as Specified,73,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,0,20000,19 - 13 Low/High,2,0.75,1630,180,>56 - 63 dBA
Elec Heated 84'' Nozzle,ECE-2-84E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-2-84E as Specified,85,ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.93,0,20000,19 - 13 Low/High,2,0.75,1630,195,>56 - 63 dBA
Elec Heated 96'' Nozzle,ECE-2-96E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-2-96E as Specified,97,ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.92,0,20000,19 - 13 Low/High,2,0.75,1630,210,>56 - 63 dBA
Elec Heated 108'' Nozzle,ECE-3-108E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-3-108E as Specified,109,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,0,30000,19 - 13 Low/High,3,0.75,1630,255,>56 - 63 dBA
Elec Heated 120'' Nozzle,ECE-3-120E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-3-120E as Specified,119,ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,30000,19 - 13 Low/High,3,0.75,1630,285,>56 - 63 dBA
Elec Heated 133'' Nozzle,ECE-3-132E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-3-132E as Specified,134,ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,30000,19 - 13 Low/High,3,0.75,1630,300,>56 - 63 dBA
Elec Heated 145'' Nozzle,ECE-4-144E,Powered Aire Electrically Heated Climate Control Air Curtain - ECE-4-144E as Specified,146,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,6800 - 10200 CFM Low/High Avg,0.95,0,40000,19 - 13 Low/High,4,0.75,1630,355,>56 - 63 dBA
