,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,HVAC_BTU Input##other##,Temperature Rise_Range##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
ECE HW Heated 36'' Nozzle,ECE-1-36HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-1-36HW as Specified,39,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.95,97000,52 - 35 Low/High,1,0.75,1630,115,56 - 63 dBA
ECE HW Heated 48'' Nozzle,ECE-1-48HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-1-48HW as Specified,51,ARI Standard 410  ;  ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.92,102000,54 - 37 Low/High,1,0.75,1630,145,56 - 63 dBA
ECE HW Heated 60'' Nozzle,ECE-1-60HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-1-60HW as Specified,63,ARI Standard 410  ;  ETL  ;  Made in USA,12,1500 - 2200 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.91,100000,54 - 36 Low/High,1,0.75,1630,180,56 - 63 dBA
ECE HW Heated 72'' Nozzle,ECE-2-72HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-2-72HW as Specified,75.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,194000,52 - 35 Low/High,2,0.75,1630,250,>56 - 63 dBA
ECE HW Heated 84'' Nozzle,ECE-2-84HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-2-84HW as Specified,87.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.93,205000,55 - 37 Low/High,2,0.75,1630,280,>56 - 63 dBA
ECE HW Heated 96'' Nozzle,ECE-2-96HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-2-96HW as Specified,99.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.92,194000,52 - 35 Low/High,2,0.75,1630,305,>56 - 63 dBA
ECE HW Heated 108'' Nozzle 2 Motor,ECE-2-108HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-2-108HW as Specified,111.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,1700 - 2500 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,192000,52 - 35 Low/High,2,0.75,1630,330,>56 - 63 dBA
ECE HW Heated 108'' Nozzle 3 Motor,ECE-3-108HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-3-108HW as Specified,111.15625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.92,283000,51 - 34 Low/High,3,0.75,1630,365,>56 - 63 dBA
ECE HW Heated 120'' Nozzle,ECE-3-120HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-3-120HW as Specified,123.15625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,307000,55 - 37 Low/High,3,0.75,1630,405,>56 - 63 dBA
ECE HW Heated 132'' Nozzle,ECE-3-132HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-3-132HW as Specified,135.15625,ARI Standard 410  ;  ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,307000,55 - 37 Low/High,3,0.75,1630,470,>56 - 63 dBA
ECE HW Heated 144'' Nozzle,ECE-4-144HW,Powered Aire Water Heated Climate Control Air Curtain - ECE-4-144HW as Specified,147.21875,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,6900 - 10200 CFM Low/High Avg,0.95,388000,52 - 35 Low/High,4,0.75,1630,490,>56 - 63 dBA
