,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,HVAC_BTU Input##other##,Temperature Rise_Range##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
ECE Steam Heated 36'' Nozzle,ECE-1-36ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-1-36ST as Specified,39,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.95,108000,58 - 39 Low/High,1,0.75,1630,115,56 - 63 dBA
ECE Steam Heated 48'' Nozzle,ECE-1-48ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-1-48ST as Specified,51,ARI Standard 410  ;  ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.92,108000,58 - 39 Low/High,1,0.75,1630,145,56 - 63 dBA
ECE Steam Heated 60'' Nozzle,ECE-1-60ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-1-60ST as Specified,63,ARI Standard 410  ;  ETL  ;  Made in USA,12,1500 - 2200 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.91,114000,61 - 41 Low/High,1,0.75,1630,180,56 - 63 dBA
ECE Steam Heated 72'' Nozzle,ECE-2-72ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-2-72ST as Specified,75.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,202000,54 - 36 Low/High,2,0.75,1630,250,>56 - 63 dBA
ECE Steam Heated 84'' Nozzle,ECE-2-84ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-2-84ST as Specified,87.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.93,210000,57 - 38 Low/High,2,0.75,1630,280,>56 - 63 dBA
ECE Steam Heated 96'' Nozzle,ECE-2-96ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-2-96ST as Specified,99.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.92,215000,58 - 39 Low/High,2,0.75,1630,305,>56 - 63 dBA
ECE Steam Heated 108'' Nozzle 2 Motor,ECE-2-108ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-2-108ST as Specified,111.0625,ARI Standard 410  ;  ETL  ;  Made in USA,12,1700 - 2500 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,198000,54 - 36 Low/High,2,0.75,1630,330,>56 - 63 dBA
ECE Steam Heated 108'' Nozzle 3 Motor,ECE-3-108ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-3-108ST as Specified,111.15625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.92,292000,52 - 35 Low/High,3,0.75,1630,365,>56 - 63 dBA
ECE Steam Heated 120'' Nozzle,ECE-3-120ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-3-120ST as Specified,123.15625,ARI Standard 410  ;  ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,305000,55 - 37 Low/High,3,0.75,1630,405,>56 - 63 dBA
ECE Steam Heated 132'' Nozzle,ECE-3-132ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-3-132ST as Specified,135.15625,ARI Standard 410  ;  ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,326000,59 - 39 Low/High,3,0.75,1630,470,>56 - 63 dBA
ECE Steam Heated 144'' Nozzle,ECE-4-144ST,Powered Aire Steam Heated Climate Control Air Curtain - ECE-4-144ST as Specified,147.21875,ARI Standard 410  ;  ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,6900 - 10200 CFM Low/High Avg,0.95,390000,52 - 35 Low/High,4,0.75,1630,490,>56 - 63 dBA
