,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,Temperature Rise_Range##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
Unheated 36'' Nozzle,ECE-1-36,Powered Aire Unheated Climate Control Air Curtain - ECE-1-36 as Specified,37,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.95,0,0,0,1,0.75,1630,90,56 - 63 dBA
Unheated 42'' Nozzle,ECE-1-42,Powered Aire Unheated Climate Control Air Curtain - ECE-1-42 as Specified,43,ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.93,0,0,0,1,0.75,1630,100,56 - 63 dBA
Unheated 48'' Nozzle,ECE-1-48,Powered Aire Unheated Climate Control Air Curtain - ECE-1-48 as Specified,49,ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,1700 - 2600 CFM Low/High Avg,0.92,0,0,0,1,0.75,1630,105,56 - 63 dBA
Unheated 60'' Nozzle 1 Motor,ECE-1-60,Powered Aire Unheated Climate Control Air Curtain - ECE-1-60 as Specified,61,ETL  ;  Made in USA,12,1500 - 2200 FPM Low/High Avg,1700 - 2500 CFM Low/High Avg,0.91,0,0,0,1,0.75,1630,120,56 - 63 dBA
Unheated 60'' Nozzle 2 Motor,ECE-2-60,Powered Aire Unheated Climate Control Air Curtain - ECE-2-60 as Specified,61,ETL  ;  Made in USA,12,2200 - 3300 FPM Low/High Avg,2600 - 3800 CFM Low/High Avg,0.94,0,0,0,2,0.75,1630,150,>56 - 63 dBA
Unheated 72'' Nozzle,ECE-2-72,Powered Aire Unheated Climate Control Air Curtain - ECE-2-72 as Specified,73,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.95,0,0,0,2,0.75,1630,170,>56 - 63 dBA
Unheated 84'' Nozzle,ECE-2-84,Powered Aire Unheated Climate Control Air Curtain - ECE-2-84 as Specified,85,ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.93,0,0,0,2,0.75,1630,190,>56 - 63 dBA
Unheated 96'' Nozzle,ECE-2-96,Powered Aire Unheated Climate Control Air Curtain - ECE-2-96 as Specified,97,ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,3400 - 5100 CFM Low/High Avg,0.92,0,0,0,2,0.75,1630,205,>56 - 63 dBA
Unheated 108'' Nozzle,ECE-3-108,Powered Aire Unheated Climate Control Air Curtain - ECE-3-108 as Specified,109,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.95,0,0,0,3,0.75,1630,245,>56 - 63 dBA
Unheated 120'' Nozzle,ECE-3-120,Powered Aire Unheated Climate Control Air Curtain - ECE-3-120 as Specified,119,ETL  ;  Made in USA,12,2100 - 3200 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,0,0,3,0.75,1630,275,>56 - 63 dBA
Unheated 133'' Nozzle,ECE-3-132,Powered Aire Unheated Climate Control Air Curtain - ECE-3-132 as Specified,134,ETL  ;  Made in USA,12,1900 - 2800 FPM Low/High Avg,5100 - 7600 CFM Low/High Avg,0.94,0,0,0,3,0.75,1630,290,>56 - 63 dBA
Unheated 145'' Nozzle,ECE-4-144,Powered Aire Unheated Climate Control Air Curtain - ECE-4-144 as Specified,146,ETL  ;  Made in USA,12,2500 - 3700 FPM Low/High Avg,6800 - 10200 CFM Low/High Avg,0.95,0,0,0,4,0.75,1630,340,>56 - 63 dBA
