,Model##Other##,Description##Other##,Unit Width##length##inches,Unit Height##length##inches,Unit Depth##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
14 ft Opening TFD 36'' Nozzle,TFD-1-36,Powered Aire Unheated Industrial Air Curtain - TFD-1-36 as Specified,39,16.75,21.25,ETL  ;  Made in USA,14,4000,3500,0.95,0,1,1.5,1725,120,66 dBA
14 ft Opening TFD 48'' Nozzle,TFD-1-48,Powered Aire Unheated Industrial Air Curtain - TFD-1-48 as Specified,51,16.75,21.25,ETL  ;  Made in USA,14,3000,3600,0.93,0,1,1.5,1725,150,66 dBA
14 ft Opening TFD 60'' Nozzle,TFD-1-60,Powered Aire Unheated Industrial Air Curtain - TFD-1-60 as Specified,63,16.75,21.25,ETL  ;  Made in USA,14,2500,3600,0.92,0,1,1.5,1725,190,66 dBA
14 ft Opening TFD 72'' Nozzle,TFD-2-72,Powered Aire Unheated Industrial Air Curtain - TFD-2-72 as Specified,75.0625,16.75,21.25,ETL  ;  Made in USA,14,4000,7100,0.95,0,2,1.5,1725,260,>66 dBA
14 ft Opening TFD 84'' Nozzle,TFD-2-84,Powered Aire Unheated Industrial Air Curtain - TFD-2-84 as Specified,87.0625,16.75,21.25,ETL  ;  Made in USA,14,3500,7100,0.93,0,2,1.5,1725,290,>66 dBA
14 ft Opening TFD 96'' Nozzle,TFD-2-96,Powered Aire Unheated Industrial Air Curtain - TFD-2-96 as Specified,99.0625,16.75,21.25,ETL  ;  Made in USA,14,3000,7100,0.92,0,2,1.5,1725,320,>66 dBA
14 ft Opening TFD 108'' Nozzle 2 Motor,TFD-2-108,Powered Aire Unheated Industrial Air Curtain - TFD-2-108 as Specified,111.0625,16.75,21.25,ETL  ;  Made in USA,14,2700,7200,0.91,0,2,1.5,1725,340,>66 dBA
14 ft Opening TFD 108'' Nozzle 3 Motor,TFD-3-108,Powered Aire Unheated Industrial Air Curtain - TFD-3-108 as Specified,111.15625,16.75,21.25,ETL  ;  Made in USA,14,4000,10600,0.95,0,3,1.5,1725,380,>66 dBA
14 ft Opening TFD 120'' Nozzle,TFD-3-120,Powered Aire Unheated Industrial Air Curtain - TFD-3-120 as Specified,123.15625,16.75,21.25,ETL  ;  Made in USA,14,3600,10600,0.94,0,3,1.5,1725,420,>66 dBA
14 ft Opening TFD 132'' Nozzle,TFD-3-132,Powered Aire Unheated Industrial Air Curtain - TFD-3-132 as Specified,135.15625,16.75,21.25,ETL  ;  Made in USA,14,3300,10700,0.95,0,3,1.5,1725,490,>66 dBA
14 ft Opening TFD 144'' Nozzle,TFD-4-144,Powered Aire Unheated Industrial Air Curtain - TFD-4-144 as Specified,147.21875,16.75,21.25,ETL  ;  Made in USA,14,4000,14200,0.95,0,4,1.5,1725,510,>66 dBA
14 ft Opening TFD 156'' Nozzle,TFD-4-156,Powered Aire Unheated Industrial Air Curtain - TFD-4-156 as Specified,159.21875,16.75,21.25,ETL  ;  Made in USA,14,3700,14200,0.94,0,4,1.5,1725,520,>66 dBA
14 ft Opening TFD 168'' Nozzle,TFD-4-168,Powered Aire Unheated Industrial Air Curtain - TFD-4-168 as Specified,171.21875,16.75,21.25,ETL  ;  Made in USA,14,3500,14200,0.95,0,4,1.5,1725,530,>66 dBA
17 ft Opening TSD 48'' Nozzle,TSD-1-48,Powered Aire Unheated Industrial Air Curtain - TSD-1-48 as Specified,51,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3900,5200,0.951,3000,1,3,1160,340,69 dBA
17 ft Opening TSD 60'' Nozzle,TSD-1-60,Powered Aire Unheated Industrial Air Curtain - TSD-1-60 as Specified,63,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3000,4900,0.92,2100,1,3,1160,380,69 dBA
17 ft Opening TSD 72'' Nozzle,TSD-1-72,Powered Aire Unheated Industrial Air Curtain - TSD-1-72 as Specified,75,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,2900,5600,0.863,2500,1,3,1160,400,69 dBA
17 ft Opening TSD 96'' Nozzle,TSD-2-96,Powered Aire Unheated Industrial Air Curtain - TSD-2-96 as Specified,99.125,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3900,10300,0.951,6000,2,3,1160,680,>69 dBA
17 ft Opening TSD 108'' Nozzle,TSD-2-108,Powered Aire Unheated Industrial Air Curtain - TSD-2-108 as Specified,111.125,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3400,10000,0.92,5100,2,3,1160,720,>69 dBA
17 ft Opening TSD 120'' Nozzle,TSD-2-120,Powered Aire Unheated Industrial Air Curtain - TSD-2-120 as Specified,123.125,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3000,9700,0.92,4200,2,3,1160,760,>69 dBA
17 ft Opening TSD 132'' Nozzle,TSD-2-132,Powered Aire Unheated Industrial Air Curtain - TSD-2-132 as Specified,135.125,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,2900,10400,0.863,4600,2,3,1160,780,>69 dBA
17 ft Opening TSD 144'' Nozzle 2 Motor,TSD-2-144,Powered Aire Unheated Industrial Air Curtain - TSD-2-144 as Specified,147.125,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,2900,11200,0.863,5000,2,3,1160,800,>69 dBA
17 ft Opening TSD 144'' Nozzle 3 Motor,TSD-3-144,Powered Aire Unheated Industrial Air Curtain - TSD-3-144 as Specified,147.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3900,15500,0.951,9000,3,3,1160,1020,>69 dBA
17 ft Opening TSD 156'' Nozzle,TSD-3-156,Powered Aire Unheated Industrial Air Curtain - TSD-3-156 as Specified,159.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3600,15200,0.92,8100,3,3,1160,1060,>69 dBA
17 ft Opening TSD 168'' Nozzle,TSD-3-168,Powered Aire Unheated Industrial Air Curtain - TSD-3-168 as Specified,171.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3500,15900,0.863,8500,3,3,1160,1080,>69 dBA
17 ft Opening TSD 180'' Nozzle,TSD-3-180,Powered Aire Unheated Industrial Air Curtain - TSD-3-180 as Specified,183.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3200,15600,0.863,7600,3,3,1160,1120,>69 dBA
17 ft Opening TSD 192'' Nozzle 3 Motor,TSD-3-192,Powered Aire Unheated Industrial Air Curtain - TSD-3-192 as Specified,195.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3100,16300,0.863,8000,3,3,1160,1140,>69 dBA
17 ft Opening TSD 204'' Nozzle 3 Motor,TSD-3-204,Powered Aire Unheated Industrial Air Curtain - TSD-3-204 as Specified,207.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,2900,16000,0.863,7100,3,3,1160,1170,>69 dBA
17 ft Opening TSD 216'' Nozzle 3 Motor,TSD-3-216,Powered Aire Unheated Industrial Air Curtain - TSD-3-216 as Specified,219.25,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,2900,16700,0.863,7500,3,3,1160,1200,>69 dBA
17 ft Opening TSD 192'' Nozzle 4 Motor,TSD-4-192,Powered Aire Unheated Industrial Air Curtain - TSD-4-192 as Specified,195.375,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3900,20700,95.1,12000,4,3,1160,1360,>69 dBA
17 ft Opening TSD 204'' Nozzle 4 Motor,TSD-4-204,Powered Aire Unheated Industrial Air Curtain - TSD-4-204 as Specified,207.375,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3600,20400,92,11100,4,3,1160,1400,>69 dBA
17 ft Opening TSD 216'' Nozzle 4 Motor,TSD-4-216,Powered Aire Unheated Industrial Air Curtain - TSD-4-216 as Specified,219.375,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3600,21100,0.863,11500,4,3,1160,1420,>69 dBA
17 ft Opening TSD 228'' Nozzle,TSD-4-228,Powered Aire Unheated Industrial Air Curtain - TSD-4-228 as Specified,231.375,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3300,20800,0.863,10600,4,3,1160,1460,>69 dBA
17 ft Opening TSD 240'' Nozzle 4 Motor,TSD-4-240,Powered Aire Unheated Industrial Air Curtain - TSD-4-240 as Specified,243.375,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3300,21500,0.863,11000,4,3,1160,1480,>69 dBA
17 ft Opening TSD 252'' Nozzle 4 Motor,TSD-4-252,Powered Aire Unheated Industrial Air Curtain - TSD-4-252 as Specified,255.375,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3100,21200,0.863,10100,4,3,1160,1510,>69 dBA
17 ft Opening TSD 240'' Nozzle 5 Motor,TSD-5-240,Powered Aire Unheated Industrial Air Curtain - TSD-5-240 as Specified,243.5,21,27.25,AMCA 220  ;  ETL  ;  Made in USA ,17,3900,25900,0.951,15000,5,3,1160,1700,>69 dBA
22 ft Opening EHD 48'' Nozzle,EHD-1-48,Powered Aire Unheated Industrial Air Curtain - EHD-1-48 as Specified,51,21,27.25,ETL  ;  Made in USA,22,5500,6300,0.95,0,1,5,1160,390,71 dBA
22 ft Opening EHD 60'' Nozzle,EHD-1-60,Powered Aire Unheated Industrial Air Curtain - EHD-1-60 as Specified,63,21,27.25,ETL  ;  Made in USA,22,4400,7500,0.94,0,1,5,1160,420,71 dBA
22 ft Opening EHD 72'' Nozzle,EHD-1-72,Powered Aire Unheated Industrial Air Curtain - EHD-1-72 as Specified,75,21,27.25,ETL  ;  Made in USA,22,5100,9300,0.94,0,1,5,1160,440,71 dBA
22 ft Opening EHD 96'' Nozzle,EHD-2-96,Powered Aire Unheated Industrial Air Curtain - EHD-2-96 as Specified,99.125,21,27.25,ETL  ;  Made in USA,22,4800,13000,0.95,0,2,5,1160,750,>71 dBA
22 ft Opening EHD 108'' Nozzle,EHD-2-108,Powered Aire Unheated Industrial Air Curtain - EHD-2-108 as Specified,111.125,21,27.25,ETL  ;  Made in USA,22,4600,13800,0.94,0,2,5,1160,780,>71 dBA
22 ft Opening EHD 120'' Nozzle,EHD-2-120,Powered Aire Unheated Industrial Air Curtain - EHD-2-120 as Specified,123.125,21,27.25,ETL  ;  Made in USA,22,4400,15800,0.94,0,2,5,1160,810,>71 dBA
22 ft Opening EHD 132'' Nozzle,EHD-2-132,Powered Aire Unheated Industrial Air Curtain - EHD-2-132 as Specified,135.125,21,27.25,ETL  ;  Made in USA,22,4800,16100,0.95,0,2,5,1160,830,>71 dBA
22 ft Opening EHD 144'' Nozzle,EHD-2-144,Powered Aire Unheated Industrial Air Curtain - EHD-2-144 as Specified,147.125,21,27.25,ETL  ;  Made in USA,22,4800,19200,0.95,0,2,5,1160,850,>71 dBA
22 ft Opening EHD 156'' Nozzle,EHD-3-156,Powered Aire Unheated Industrial Air Curtain - EHD-3-156 as Specified,159.25,21,27.25,ETL  ;  Made in USA,22,4700,20300,0.94,0,3,5,1160,1150,>71 dBA
22 ft Opening EHD 168'' Nozzle,EHD-3-168,Powered Aire Unheated Industrial Air Curtain - EHD-3-168 as Specified,171.25,21,27.25,ETL  ;  Made in USA,22,4500,22800,0.94,0,3,5,1160,1180,>71 dBA
22 ft Opening EHD 180'' Nozzle,EHD-3-180,Powered Aire Unheated Industrial Air Curtain - EHD-3-180 as Specified,183.25,21,27.25,ETL  ;  Made in USA,22,4400,23000,0.94,0,3,5,1160,1210,>71 dBA
22 ft Opening EHD 192'' Nozzle,EHD-3-192,Powered Aire Unheated Industrial Air Curtain - EHD-3-192 as Specified,195.25,21,27.25,ETL  ;  Made in USA,22,4800,23300,0.95,0,3,5,1160,1230,>71 dBA
22 ft Opening EHD 204'' Nozzle,EHD-3-204,Powered Aire Unheated Industrial Air Curtain - EHD-3-204 as Specified,207.25,21,27.25,ETL  ;  Made in USA,22,4400,23400,0.94,0,3,5,1160,1250,>71 dBA
22 ft Opening EHD 216'' Nozzle,EHD-3-216,Powered Aire Unheated Industrial Air Curtain - EHD-3-216 as Specified,219.25,21,27.25,ETL  ;  Made in USA,22,4600,24600,0.95,0,3,5,1160,1270,>71 dBA
22 ft Opening EHD 228'' Nozzle,EHD-4-228,Powered Aire Unheated Industrial Air Curtain - EHD-4-228 as Specified,231.375,21,27.25,ETL  ;  Made in USA,22,4800,28300,0.94,0,4,5,1160,1620,>71 dBA
22 ft Opening EHD 240'' Nozzle,EHD-4-240,Powered Aire Unheated Industrial Air Curtain - EHD-4-240 as Specified,243.375,21,27.25,ETL  ;  Made in USA,22,4400,29100,0.95,0,4,5,1160,1650,>71 dBA
30 ft Opening BPA 60'' Nozzle,BPA-1-60,Powered Aire Unheated Industrial Air Curtain - BPA-1-60 as Specified,63,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4000,9700,0.94,0,1,7.5,1160,470,73 dBA
30 ft Opening BPA 72'' Nozzle,BPA-1-72,Powered Aire Unheated Industrial Air Curtain - BPA-1-72 as Specified,75,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4300,12000,0.94,0,1,7.5,1160,490,73 dBA
30 ft Opening BPA 84'' Nozzle,BPA-1-84,Powered Aire Unheated Industrial Air Curtain - BPA-1-84 as Specified,87,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4000,13100,0.92,0,1,7.5,1160,530,73 dBA
30 ft Opening BPA 120'' Nozzle,BPA-2-120,Powered Aire Unheated Industrial Air Curtain - BPA-2-120 as Specified,123.125,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4400,20500,0.94,0,2,7.5,1160,900,>73 dBA
30 ft Opening BPA 132'' Nozzle,BPA-2-132,Powered Aire Unheated Industrial Air Curtain - BPA-2-132 as Specified,135.125,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4100,21000,0.95,0,2,7.5,1160,930,>73 dBA
30 ft Opening BPA 144'' Nozzle,BPA-2-144,Powered Aire Unheated Industrial Air Curtain - BPA-2-144 as Specified,147.125,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4400,25000,0.95,0,2,7.5,1160,950,>73 dBA
30 ft Opening BPA 156'' Nozzle,BPA-2-156,Powered Aire Unheated Industrial Air Curtain - BPA-2-156 as Specified,159.125,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4300,26300,0.92,0,2,7.5,1160,1000,>73 dBA
30 ft Opening BPA 168'' Nozzle,BPA-2-168,Powered Aire Unheated Industrial Air Curtain - BPA-2-168 as Specified,171.125,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4500,29700,0.92,0,2,7.5,1160,1040,>73 dBA
30 ft Opening BPA 180'' Nozzle,BPA-3-180,Powered Aire Unheated Industrial Air Curtain - BPA-3-180 as Specified,183.25,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4300,29900,0.94,0,3,7.5,1160,1340,>73 dBA
30 ft Opening BPA 192'' Nozzle,BPA-3-192,Powered Aire Unheated Industrial Air Curtain - BPA-3-192 as Specified,195.25,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4100,30300,0.95,0,3,7.5,1160,1360,>73 dBA
30 ft Opening BPA 204'' Nozzle,BPA-3-204,Powered Aire Unheated Industrial Air Curtain - BPA-3-204 as Specified,207.25,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,3800,30400,0.94,0,3,7.5,1160,1370,>73 dBA
30 ft Opening BPA 216'' Nozzle,BPA-3-216,Powered Aire Unheated Industrial Air Curtain - BPA-3-216 as Specified,219.25,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,3800,32000,0.95,0,3,7.5,1160,1410,>73 dBA
30 ft Opening BPA 228'' Nozzle,BPA-3-228,Powered Aire Unheated Industrial Air Curtain - BPA-3-228 as Specified,231.25,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4200,36800,0.94,0,3,7.5,1160,1460,>73 dBA
30 ft Opening BPA 240'' Nozzle 3 Motor,BPA-3-240,Powered Aire Unheated Industrial Air Curtain - BPA-3-240 as Specified,243.25,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4100,37900,0.92,0,3,7.5,1160,1510,>73 dBA
30 ft Opening BPA 240'' Nozzle 4 Motor,BPA-4-240,Powered Aire Unheated Industrial Air Curtain - BPA-4-240 as Specified,243.375,25,33.625,ETL  ;  Made in USA  ;  Hazardous and Corrosive Duty Capable,30,4300,40200,0.95,0,4,7.5,1160,1800,>73 dBA
50 ft Opening XPA 72'' Nozzle,XPA-1-72,Powered Aire Unheated Industrial Air Curtain - XPA-1-72 as Specified,75,30,40,Made in USA,50,5400,21800,0.93,0,1,20,1175,900,85 dBA
50 ft Opening XPA 84'' Nozzle,XPA-1-84,Powered Aire Unheated Industrial Air Curtain - XPA-1-84 as Specified,87,30,40,Made in USA,50,5200,24100,0.91,0,1,20,1175,1000,85 dBA
50 ft Opening XPA 96'' Nozzle,XPA-1-96,Powered Aire Unheated Industrial Air Curtain - XPA-1-96 as Specified,99,30,40,Made in USA,50,5000,26600,0.89,0,1,20,1175,1100,85 dBA
50 ft Opening XPA 144'' Nozzle,XPA-2-144,Powered Aire Unheated Industrial Air Curtain - XPA-2-144 as Specified,147.125,30,40,Made in USA,50,5400,43600,0.93,0,2,20,1175,1800,>85 dBA
50 ft Opening XPA 156'' Nozzle,XPA-2-156,Powered Aire Unheated Industrial Air Curtain - XPA-2-156 as Specified,159.125,30,40,Made in USA,50,5300,45900,0.92,0,2,20,1175,1900,>85 dBA
50 ft Opening XPA 168'' Nozzle,XPA-2-168,Powered Aire Unheated Industrial Air Curtain - XPA-2-168 as Specified,171.125,30,40,Made in USA,50,5200,48200,0.91,0,2,20,1175,2000,>85 dBA
50 ft Opening XPA 180'' Nozzle,XPA-2-180,Powered Aire Unheated Industrial Air Curtain - XPA-2-180 as Specified,183.125,30,40,Made in USA,50,5100,50700,0.9,0,2,20,1175,2100,>85 dBA
50 ft Opening XPA 192'' Nozzle,XPA-2-192,Powered Aire Unheated Industrial Air Curtain - XPA-2-192 as Specified,195.125,30,40,Made in USA,50,5000,53200,0.89,0,2,20,1175,2200,>85 dBA
50 ft Opening XPA 216'' Nozzle,XPA-3-216,Powered Aire Unheated Industrial Air Curtain - XPA-3-216 as Specified,219.25,30,40,Made in USA,50,5400,65400,0.93,0,3,20,1175,2700,>85 dBA
50 ft Opening XPA 228'' Nozzle,XPA-3-228,Powered Aire Unheated Industrial Air Curtain - XPA-3-228 as Specified,231.25,30,40,Made in USA,50,5300,67700,0.92,0,3,20,1175,2800,>85 dBA
50 ft Opening XPA 240'' Nozzle,XPA-3-240,Powered Aire Unheated Industrial Air Curtain - XPA-3-240 as Specified,243.25,30,40,Made in USA,50,5200,70000,0.91,0,3,20,1175,2900,>85 dBA
50 ft Opening XPA 252'' Nozzle,XPA-3-252,Powered Aire Unheated Industrial Air Curtain - XPA-3-252 as Specified,255.25,30,40,Made in USA,50,5200,72300,0.91,0,3,20,1175,3000,>85 dBA
50 ft Opening XPA 264'' Nozzle,XPA-3-264,Powered Aire Unheated Industrial Air Curtain - XPA-3-264 as Specified,267.25,30,40,Made in USA,50,5100,74800,0.9,0,3,20,1175,3100,>85 dBA
50 ft Opening XPA 276'' Nozzle,XPA-3-276,Powered Aire Unheated Industrial Air Curtain - XPA-3-276 as Specified,279.25,30,40,Made in USA,50,5100,77300,0.9,0,3,20,1175,3200,>85 dBA
50 ft Opening XPA 288'' Nozzle,XPA-3-288,Powered Aire Unheated Industrial Air Curtain - XPA-3-288 as Specified,291.25,30,40,Made in USA,50,5000,79800,0.89,0,3,20,1175,3300,>85 dBA
50 ft Opening XPA 300'' Nozzle,XPA-4-300,Powered Aire Unheated Industrial Air Curtain - XPA-4-300 as Specified,303.375,30,40,Made in USA,50,5400,89500,0.92,0,4,20,1175,3700,>85 dBA
50 ft Opening XPA 312'' Nozzle,XPA-4-312,Powered Aire Unheated Industrial Air Curtain - XPA-4-312 as Specified,315.375,30,40,Made in USA,50,5300,91800,0.92,0,4,20,1175,3800,>85 dBA
50 ft Opening XPA 324'' Nozzle,XPA-4-324,Powered Aire Unheated Industrial Air Curtain - XPA-4-324 as Specified,327.375,30,40,Made in USA,50,5200,94100,0.92,0,4,20,1175,3900,>85 dBA
50 ft Opening XPA 336'' Nozzle,XPA-4-336,Powered Aire Unheated Industrial Air Curtain - XPA-4-336 as Specified,339.375,30,40,Made in USA,50,5200,96400,0.91,0,4,20,1175,4000,>85 dBA
50 ft Opening XPA 348'' Nozzle,XPA-4-348,Powered Aire Unheated Industrial Air Curtain - XPA-4-348 as Specified,351.375,30,40,Made in USA,50,5100,98900,0.9,0,4,20,1175,4100,>85 dBA
50 ft Opening XPA 360'' Nozzle,XPA-4-360,Powered Aire Unheated Industrial Air Curtain - XPA-4-360 as Specified,363.375,30,40,Made in USA,50,5100,101400,0.9,0,4,20,1175,4200,>85 dBA
