,Model##Other##,Description##Other##,Unit Width##length##inches,Unit Height##length##inches,Unit Depth##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,HVAC_BTU Input##other##,HVAC_Temperature Rise##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
14 ft Opening TFD 36'' Nozzle,TFD-1-36ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-1-36ST as Specified,39,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,4000,3500,0.95,136000,35,1,1.5,1725,170,66 dBA
14 ft Opening TFD 48'' Nozzle,TFD-1-48ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-1-48ST as Specified,51,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3000,3600,0.93,133000,34,1,1.5,1725,180,66 dBA
14 ft Opening TFD 60'' Nozzle,TFD-1-60ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-1-60ST as Specified,63,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,2500,3600,0.92,140000,35,1,1.5,1725,210,66 dBA
14 ft Opening TFD 72'' Nozzle,TFD-2-72ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-2-72ST as Specified,75.0625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,4000,7100,0.95,263000,34,2,1.5,1725,340,>66 dBA
14 ft Opening TFD 84'' Nozzle,TFD-2-84ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-2-84ST as Specified,87.0625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3500,7100,0.93,270000,34,2,1.5,1725,350,>66 dBA
14 ft Opening TFD 96'' Nozzle,TFD-2-96ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-2-96ST as Specified,99.0625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3000,7100,0.92,270000,34,2,1.5,1725,360,>66 dBA
14 ft Opening TFD 108'' Nozzle 2 Motor,TFD-2-108ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-2-108ST as Specified,111.0625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,2700,7200,0.91,266000,34,2,1.5,1725,380,>66 dBA
14 ft Opening TFD 108'' Nozzle 3 Motor,TFD-3-108ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-3-108ST as Specified,111.15625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,4000,10600,0.95,395000,34,3,1.5,1725,500,>66 dBA
14 ft Opening TFD 120'' Nozzle,TFD-3-120ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-3-120ST as Specified,123.15625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3600,10600,0.94,393000,33,3,1.5,1725,520,>66 dBA
14 ft Opening TFD 132'' Nozzle,TFD-3-132ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-3-132ST as Specified,135.15625,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3300,10700,0.95,414000,35,3,1.5,1725,530,>66 dBA
14 ft Opening TFD 144'' Nozzle,TFD-4-144ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-4-144ST as Specified,147.21875,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,4000,14200,0.95,551000,35,4,1.5,1725,670,>66 dBA
14 ft Opening TFD 156'' Nozzle,TFD-4-156ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-4-156ST as Specified,159.21875,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3700,14200,0.94,554000,35,4,1.5,1725,680,>66 dBA
14 ft Opening TFD 168'' Nozzle,TFD-4-168ST,Powered Aire Steam Heated Industrial Air Curtain - TFD-4-168ST as Specified,171.21875,16.75,21.25,ARI Standard 410  ;  ETL  ;  Made in USA,14,3500,14200,0.95,554000,35,4,1.5,1725,690,>66 dBA
17 ft Opening TSD 48'' Nozzle,TSD-1-48ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-1-48ST as Specified,51,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3900,5200,0.951,218000,44,1,3,1160,420,69 dBA
17 ft Opening TSD 60'' Nozzle,TSD-1-60ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-1-60ST as Specified,63,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3000,4900,0.92,243000,46,1,3,1160,470,69 dBA
17 ft Opening TSD 72'' Nozzle,TSD-1-72ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-1-72ST as Specified,75,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,2900,5600,0.863,261000,43,1,3,1160,510,69 dBA
17 ft Opening TSD 96'' Nozzle,TSD-2-96ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-2-96ST as Specified,99.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3900,10300,0.951,427000,43,2,3,1160,830,>69 dBA
17 ft Opening TSD 108'' Nozzle,TSD-2-108ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-2-108ST as Specified,111.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3400,10000,0.92,441000,43,2,3,1160,890,>69 dBA
17 ft Opening TSD 120'' Nozzle,TSD-2-120ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-2-120ST as Specified,123.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3000,9700,0.92,487000,46,2,3,1160,940,>69 dBA
17 ft Opening TSD 132'' Nozzle,TSD-2-132ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-2-132ST as Specified,135.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,2900,10400,0.863,489000,43,2,3,1160,980,>69 dBA
17 ft Opening TSD 144'' Nozzle 2 Motor,TSD-2-144ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-2-144ST as Specified,147.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,2900,11200,0.863,547000,45,2,3,1160,1020,>69 dBA
17 ft Opening TSD 144'' Nozzle 3 Motor,TSD-3-144ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-3-144ST as Specified,147.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3900,15500,0.951,547000,37,3,3,1160,1240,>69 dBA
17 ft Opening TSD 156'' Nozzle,TSD-3-156ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-3-156ST as Specified,159.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3600,15200,0.92,670000,44,3,3,1160,1300,>69 dBA
17 ft Opening TSD 168'' Nozzle,TSD-3-168ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-3-168ST as Specified,171.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3500,15900,0.863,704000,44,3,3,1160,1340,>69 dBA
17 ft Opening TSD 180'' Nozzle,TSD-3-180ST,Powered Aire Steam Heated Industrial Air Curtain - TSD-3-180ST as Specified,183.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,17,3200,15600,0.863,702000,43,3,3,1160,1400,>69 dBA
22 ft Opening EHD 48'' Nozzle,EHD-1-48ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-1-48ST as Specified,51,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,5500,6300,0.95,302000,44,1,5,1160,460,71 dBA
22 ft Opening EHD 60'' Nozzle,EHD-1-60ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-1-60ST as Specified,63,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4400,7500,0.94,365000,46,1,5,1160,520,71 dBA
22 ft Opening EHD 72'' Nozzle,EHD-1-72ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-1-72ST as Specified,75,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,5100,9300,0.94,434000,43,1,5,1160,560,71 dBA
22 ft Opening EHD 96'' Nozzle,EHD-2-96ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-2-96ST as Specified,99.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4800,13000,0.95,608000,43,2,5,1160,900,>71 dBA
22 ft Opening EHD 108'' Nozzle,EHD-2-108ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-2-108ST as Specified,111.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4600,13800,0.94,645000,43,2,5,1160,960,>71 dBA
22 ft Opening EHD 120'' Nozzle,EHD-2-120ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-2-120ST as Specified,123.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4400,15800,0.94,730000,46,2,5,1160,1010,>71 dBA
22 ft Opening EHD 132'' Nozzle,EHD-2-132ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-2-132ST as Specified,135.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4800,16100,0.95,852000,43,2,5,1160,1030,>71 dBA
22 ft Opening EHD 144'' Nozzle,EHD-2-144ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-2-144ST as Specified,147.125,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4800,19200,0.95,852000,43,2,5,1160,1070,>71 dBA
22 ft Opening EHD 156'' Nozzle,EHD-3-156ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-3-156ST as Specified,159.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4700,20300,0.94,972000,44,3,5,1160,1340,>71 dBA
22 ft Opening EHD 168'' Nozzle,EHD-3-168ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-3-168ST as Specified,171.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4500,22800,0.94,1032000,45,3,5,1160,1390,>71 dBA
22 ft Opening EHD 180'' Nozzle,EHD-3-180ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-3-180ST as Specified,183.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4400,23000,0.94,1071000,45,3,5,1160,1450,>71 dBA
22 ft Opening EHD 192'' Nozzle,EHD-3-192ST,Powered Aire Steam Heated Industrial Air Curtain - EHD-3-192ST as Specified,195.25,21,27.25,ARI Standard 410  ;  ETL  ;  Made in USA ,22,4800,23300,0.95,1094000,43,3,5,1160,1480,>71 dBA
