,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,HVAC_Temperature Rise##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
Unheated 36'' Nozzle,CHA-1-36,Powered Aire Unheated Vestible Exception Air Curtain - CHA-1-36 as Specified,39,AMCA  220;  ETL  ;  Made in USA,14,3000,1400,0.91,680,0,0,1,0.75,1630,180,63 dBA
Unheated 48'' Nozzle,CHA-1-48,Powered Aire Unheated Vestible Exception Air Curtain - CHA-1-48 as Specified,51,AMCA  220;  ETL  ;  Made in USA,14,2700,1800,0.91,840,0,0,1,0.75,1630,200,63 dBA
Unheated 60'' Nozzle,CHA-1-60,Powered Aire Unheated Vestible Exception Air Curtain - CHA-1-60 as Specified,63,AMCA  220;  ETL  ;  Made in USA,14,2400,1800,0.73,870,0,0,1,0.75,1630,230,63 dBA
Unheated 72'' Nozzle,CHA-2-72,Powered Aire Unheated Vestible Exception Air Curtain - CHA-2-72 as Specified,75.0625,AMCA  220;  ETL  ;  Made in USA,14,3000,2700,0.91,1360,0,0,2,0.75,1630,360,>63 dBA
Unheated 84'' Nozzle,CHA-2-84,Powered Aire Unheated Vestible Exception Air Curtain - CHA-2-84 as Specified,87.0625,AMCA  220;  ETL  ;  Made in USA,14,2800,3100,0.91,1520,0,0,2,0.75,1630,370,>63 dBA
Unheated 96'' Nozzle,CHA-2-96,Powered Aire Unheated Vestible Exception Air Curtain - CHA-2-96 as Specified,99.0625,AMCA  220;  ETL  ;  Made in USA,14,2700,3500,0.91,1680,0,0,2,0.75,1630,380,>63 dBA
Unheated 108'' Nozzle 2 Motor,CHA-2-108,Powered Aire Unheated Vestible Exception Air Curtain - CHA-2-108 as Specified,111.0625,AMCA  220;  ETL  ;  Made in USA,14,2500,3600,0.73,1710,0,0,2,0.75,1630,400,>63 dBA
Unheated 108'' Nozzle 3 Motor,CHA-3-108,Powered Aire Unheated Vestible Exception Air Curtain - CHA-3-108 as Specified,111.15625,AMCA  220;  ETL  ;  Made in USA,14,3000,4100,0.91,2040,0,0,3,0.75,1630,540,>63 dBA
Unheated 120'' Nozzle,CHA-3-120,Powered Aire Unheated Vestible Exception Air Curtain - CHA-3-120 as Specified,123.15625,AMCA  220;  ETL  ;  Made in USA,14,2900,4500,0.73,2200,0,0,3,0.75,1630,550,>63 dBA
Unheated 132'' Nozzle,CHA-3-132,Powered Aire Unheated Vestible Exception Air Curtain - CHA-3-132 as Specified,135.15625,AMCA  220;  ETL  ;  Made in USA,14,2800,4900,0.91,2360,0,0,3,0.75,1630,560,>63 dBA
Unheated 144'' Nozzle,CHA-4-144,Powered Aire Unheated Vestible Exception Air Curtain - CHA-4-144 as Specified,147.21875,AMCA  220;  ETL  ;  Made in USA,14,3000,5500,0.91,2520,0,0,4,0.75,1630,720,>63 dBA
Elec Heated 36'' Nozzle,CHA-1-36E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-1-36E as Specified,39,AMCA  220;  ETL  ;  Made in USA,14,2400,1200,0.86,590,10000,26.7,1,0.75,1630,180,63 dBA
Elec Heated 48'' Nozzle,CHA-1-48E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-1-48E as Specified,51,AMCA  220;  ETL  ;  Made in USA,14,2300,1500,0.79,700,10000,20.7,1,0.75,1630,200,63 dBA
Elec Heated 60'' Nozzle,CHA-1-60E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-1-60E as Specified,63,AMCA  220;  ETL  ;  Made in USA,14,1900,1600,0.82,730,10000,20,1,0.75,1630,230,63 dBA
Elec Heated 72'' Nozzle,CHA-2-72E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-2-72E as Specified,75.0625,AMCA  220;  ETL  ;  Made in USA,14,2400,2400,0.86,1180,20000,26.7,2,0.75,1630,360,>63 dBA
Elec Heated 84'' Nozzle,CHA-2-84E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-2-84E as Specified,87.0625,AMCA  220;  ETL  ;  Made in USA,14,2400,2700,0.79,1290,20000,23.3,2,0.75,1630,380,>63 dBA
Elec Heated 96'' Nozzle,CHA-2-96E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-2-96E as Specified,99.0625,AMCA  220;  ETL  ;  Made in USA,14,2300,3100,0.79,1400,20000,20.7,2,0.75,1630,400,>63 dBA
Elec Heated 108'' Nozzle 2 Motor,CHA-2-108E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-2-108E as Specified,111.0625,AMCA  220;  ETL  ;  Made in USA,14,2100,3100,0.79,1430,20000,20.3,2,0.75,1630,420,>63 dBA
Elec Heated 108'' Nozzle 3 Motor,CHA-3-108E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-3-108E as Specified,111.15625,AMCA  220;  ETL  ;  Made in USA,14,2400,3600,0.86,1770,30000,26.7,3,0.75,1630,550,>63 dBA
Elec Heated 120'' Nozzle,CHA-3-120E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-3-120E as Specified,123.15625,AMCA  220;  ETL  ;  Made in USA,14,2400,3900,0.79,1880,30000,24.3,3,0.75,1630,570,>63 dBA
Elec Heated 132'' Nozzle,CHA-3-132E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-3-132E as Specified,135.15625,AMCA  220;  ETL  ;  Made in USA,14,2400,4300,0.79,1990,30000,22.4,3,0.75,1630,580,>63 dBA
Elec Heated 144'' Nozzle,CHA-4-144E,Powered Aire Electrically Heated Vestible Exception Air Curtain - CHA-4-144E as Specified,147.21875,AMCA  220;  ETL  ;  Made in USA,14,2400,4800,0.86,2360,40000,26.7,4,0.75,1630,730,>63 dBA
