,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Heating Element Load##other##,HVAC_Temperature Rise##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
Unheated 36'' Nozzle,ETA-1-36,Powered Aire Unheated Vestible Exception Air Curtain - ETA-1-36 as Specified,37,AMCA 220  ;  ETL  ;  Made in USA,14,2100,1400,0.88,760,0,0,1,0.75,1630,90,63 dBA
Unheated 42'' Nozzle,ETA-1-42,Powered Aire Unheated Vestible Exception Air Curtain - ETA-1-42 as Specified,43,AMCA 220  ;  ETL  ;  Made in USA,14,2000,1700,0.88,840,0,0,1,0.75,1630,100,63 dBA
Unheated 48'' Nozzle,ETA-1-48,Powered Aire Unheated Vestible Exception Air Curtain - ETA-1-48 as Specified,49,AMCA 220  ;  ETL  ;  Made in USA,14,1800,1800,0.84,860,0,0,1,0.75,1630,100,63 dBA
Unheated 60'' Nozzle,ETA-1-60,Powered Aire Unheated Vestible Exception Air Curtain - ETA-1-60 as Specified,61,AMCA 220  ;  ETL  ;  Made in USA,14,1600,2000,0.72,940,0,0,1,0.75,1630,120,63 dBA
Unheated 72'' Nozzle,ETA-2-72,Powered Aire Unheated Vestible Exception Air Curtain - ETA-2-72 as Specified,73,AMCA 220  ;  ETL  ;  Made in USA,14,2100,2800,0.88,1520,0,0,2,0.75,1630,170,>63 dBA
Unheated 84'' Nozzle,ETA-2-84,Powered Aire Unheated Vestible Exception Air Curtain - ETA-2-84 as Specified,85,AMCA 220  ;  ETL  ;  Made in USA,14,2000,3400,0.88,1680,0,0,2,0.75,1630,190,>63 dBA
Unheated 96'' Nozzle,ETA-2-96,Powered Aire Unheated Vestible Exception Air Curtain - ETA-2-96 as Specified,97,AMCA 220  ;  ETL  ;  Made in USA,14,1800,3500,0.84,1720,0,0,2,0.75,1630,200,>63 dBA
Unheated 108'' Nozzle,ETA-3-108,Powered Aire Unheated Vestible Exception Air Curtain - ETA-3-108 as Specified,109,AMCA 220  ;  ETL  ;  Made in USA,14,2100,4200,0.88,2280,0,0,3,0.75,1630,250,>63 dBA
Unheated 118'' Nozzle,ETA-3-120,Powered Aire Unheated Vestible Exception Air Curtain - ETA-3-120 as Specified,119,AMCA 220  ;  ETL  ;  Made in USA,14,2000,4800,0.88,2440,0,0,3,0.75,1630,270,>63 dBA
Unheated 133'' Nozzle,ETA-3-132,Powered Aire Unheated Vestible Exception Air Curtain - ETA-3-132 as Specified,134,AMCA 220  ;  ETL  ;  Made in USA,14,1900,4800,0.72,2460,0,0,3,0.75,1630,290,>63 dBA
Unheated 145'' Nozzle,ETA-4-144,Powered Aire Unheated Vestible Exception Air Curtain - ETA-4-144 as Specified,146,AMCA 220  ;  ETL  ;  Made in USA,14,2100,5600,0.88,3040,0,0,4,0.75,1630,340,>63 dBA
Unheated 157'' Nozzle,ETA-4-156,Powered Aire Unheated Vestible Exception Air Curtain - ETA-4-156 as Specified,158,AMCA 220  ;  ETL  ;  Made in USA,14,2000,6200,0.88,3200,0,0,4,0.75,1630,360,>63 dBA
Unheated 169'' Nozzle,ETA-4-168,Powered Aire Unheated Vestible Exception Air Curtain - ETA-4-168 as Specified,170,AMCA 220  ;  ETL  ;  Made in USA,14,2000,6700,0.88,3360,0,0,4,0.75,1630,370,>63 dBA
Elec Heated 36'' Nozzle,ETA-1-36E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-1-36E as Specified,37,AMCA 220  ;  ETL  ;  Made in USA,14,1800,1300,0.82,680,10000,24.4,1,0.75,1630,95,63 dBA
Elec Heated 42'' Nozzle,ETA-1-42E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-1-42E as Specified,43,AMCA 220  ;  ETL  ;  Made in USA,14,1900,1500,0.83,710,10000,21.2,1,0.75,1630,100,63 dBA
Elec Heated 48'' Nozzle,ETA-1-48E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-1-48E as Specified,49,AMCA 220  ;  ETL  ;  Made in USA,14,1500,1400,0.85,720,10000,22.2,1,0.75,1630,110,63 dBA
Elec Heated 60'' Nozzle,ETA-1-60E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-1-60E as Specified,61,AMCA 220  ;  ETL  ;  Made in USA,14,1300,1700,0.79,780,10000,19.2,1,0.75,1630,120,63 dBA
Elec Heated 72'' Nozzle,ETA-2-72E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-2-72E as Specified,73,AMCA 220  ;  ETL  ;  Made in USA,14,1800,2600,0.82,1360,20000,24.4,2,0.75,1630,180,>63 dBA
Elec Heated 84'' Nozzle,ETA-2-84E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-2-84E as Specified,85,AMCA 220  ;  ETL  ;  Made in USA,14,1900,3000,0.83,1420,20000,21.1,2,0.75,1630,200,>63 dBA
Elec Heated 96'' Nozzle,ETA-2-96E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-2-96E as Specified,97,AMCA 220  ;  ETL  ;  Made in USA,14,1500,2900,0.85,1440,20000,22.2,2,0.75,1630,210,>63 dBA
Elec Heated 108'' Nozzle,ETA-3-108E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-3-108E as Specified,109,AMCA 220  ;  ETL  ;  Made in USA,14,1800,4000,0.82,2040,30000,24.4,3,0.75,1630,260,>63 dBA
Elec Heated 118'' Nozzle,ETA-3-120E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-3-120E as Specified,119,AMCA 220  ;  ETL  ;  Made in USA,14,1900,4300,0.82,2100,30000,22.2,3,0.75,1630,280,>63 dBA
Elec Heated 133'' Nozzle,ETA-3-132E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-3-132E as Specified,134,AMCA 220  ;  ETL  ;  Made in USA,14,1600,4300,0.79,2140,30000,22.4,3,0.75,1630,300,>63 dBA
Elec Heated 145'' Nozzle,ETA-4-144E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-4-144E as Specified,146,AMCA 220  ;  ETL  ;  Made in USA,14,1800,5200,0.82,2720,40000,24.4,4,0.75,1630,350,>63 dBA
Elec Heated 157'' Nozzle,ETA-4-156E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-4-156E as Specified,158,AMCA 220  ;  ETL  ;  Made in USA,14,1900,5600,0.82,2780,40000,22.7,4,0.75,1630,370,>63 dBA
Elec Heated 169'' Nozzle,ETA-4-168E,Powered Aire Electrically Heated Vestible Exception Air Curtain - ETA-4-168E as Specified,170,AMCA 220  ;  ETL  ;  Made in USA,14,1900,6000,0.83,2840,40000,21.2,4,0.75,1630,390,>63 dBA
