,Model##Other##,Description##Other##,Unit Width##length##inches,Nozzle Width##length##inches,Outlet Velocity_Range##other##,Outlet Volume_Range##other##,HVAC_Outlet Velocity Uniformity##other##,Temperature Rise_Range##other##,Motor Count##other##,Unit Weight##other##
Elec Heated 35'' Nozzle,EVE-1-36E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-1-36E as Specified,37,35,1316 FPM,961 CFM,0.87,27,1,59
Elec Heated 41'' Nozzle,EVE-1-42E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-1-42E as Specified,43,41,3269 FPM,1100 CFM,0.75,23,1,69
Elec Heated 48'' Nozzle,EVE-1-48E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-1-48E as Specified,49,48,3256 FPM,1344 CFM,0.85,38,1,77
Elec Heated 59'' Nozzle,EVE-1-60E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-1-60E as Specified,61,59,3218 FPM,1715 CFM,0.83,30,1,91
Elec Heated 71'' Nozzle,EVE-2-72E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-2-72E as Specified,73,71,3262 FPM,1922 CFM,0.87,27,2,102
Elec Heated 83'' Nozzle,EVE-2-84E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-2-84E as Specified,85,83,3269 FPM,2200 CFM,0.75,35,2,115
Elec Heated 95'' Nozzle,EVE-2-96E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-2-96E as Specified,97,95,3256 FPM,2688 CFM,0.85,38,2,123
Elec Heated 107'' Nozzle,EVE-2-108E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-2-108E as Specified,109,107,3242 FPM,3059 CFM,0.83,33,2,139
Elec Heated 117'' Nozzle,EVE-2-120E,Powered Aire Electrically Heated Climate Control Air Curtain - EVE-2-120E as Specified,119,117,3218 FPM,3430 CFM,0.83,30,2,152
