,Model##Other##,Description##Other##,Unit Width##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,Power Rating##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Sound Pressure##other##
36'' Nozzle,LDC-1-36,Powered Aire Unheated Corrosive Area Air Curtain - LDC-1-36 as Specified,37,Corrosive Area  ;  Made in USA,12,4218,2900,0.95,0,1,0.75,1725,90,63 dBA
42'' Nozzle,LDC-1-42,Powered Aire Unheated Corrosive Area Air Curtain - LDC-1-42 as Specified,43,Corrosive Area  ;  Made in USA,12,4218,3400,0.93,0,1,0.75,1725,100,63 dBA
48'' Nozzle,LDC-1-48,Powered Aire Unheated Corrosive Area Air Curtain - LDC-1-48 as Specified,49,Corrosive Area  ;  Made in USA,12,4218,3900,0.92,0,1,0.75,1725,105,63 dBA
60'' Nozzle,LDC-1-60,Powered Aire Unheated Corrosive Area Air Curtain - LDC-1-60 as Specified,61,Corrosive Area  ;  Made in USA,12,4218,4400,0.91,0,1,0.75,1725,120,63 dBA
72'' Nozzle,LDC-2-72,Powered Aire Unheated Corrosive Area Air Curtain - LDC-2-72 as Specified,73,Corrosive Area  ;  Made in USA,12,4218,5800,0.95,0,2,0.75,1725,170,>63 dBA
84'' Nozzle,LDC-2-84,Powered Aire Unheated Corrosive Area Air Curtain - LDC-2-84 as Specified,85,Corrosive Area  ;  Made in USA,12,4218,6800,0.93,0,2,0.75,1725,190,>63 dBA
96'' Nozzle,LDC-2-96,Powered Aire Unheated Corrosive Area Air Curtain - LDC-2-96 as Specified,97,Corrosive Area  ;  Made in USA,12,4218,7700,0.92,0,2,0.75,1725,205,>63 dBA
108'' Nozzle,LDC-3-108,Powered Aire Unheated Corrosive Area Air Curtain - LDC-3-108 as Specified,109,Corrosive Area  ;  Made in USA,12,4218,8700,0.95,0,3,0.75,1725,245,>63 dBA
118'' Nozzle,LDC-3-120,Powered Aire Unheated Corrosive Area Air Curtain - LDC-3-120 as Specified,119,Corrosive Area  ;  Made in USA,12,4218,9700,0.94,0,3,0.75,1725,275,>63 dBA
133'' Nozzle,LDC-3-132,Powered Aire Unheated Corrosive Area Air Curtain - LDC-3-132 as Specified,134,Corrosive Area  ;  Made in USA,12,4218,10900,0.95,0,3,0.75,1725,290,>63 dBA
145'' Nozzle,LDC-4-144,Powered Aire Unheated Corrosive Area Air Curtain - LDC-4-144 as Specified,146,Corrosive Area  ;  Made in USA,12,4218,11600,0.95,0,4,0.75,1725,340,>63 dBA
