,Model##Other##,Description##Other##,Unit Width##length##inches,Unit Height##length##inches,Unit Depth##length##inches,Overall Depth##length##inches,Standards Conformance##other##,Max Height##length##feet,HVAC_Outlet Velocity##other##,HVAC_Outlet Volume##other##,HVAC_Outlet Velocity Uniformity##other##,HVAC_BTU Input##other##,HVAC_BTU Output##other##,HVAC_Temperature Rise##other##,Motor Count##other##,Motor HP##other##,Motor RPM##other##,Unit Weight##other##,Heater Weight##other##,Heater Hanging Width##length##inches,Exhaust Connection Diameter##length##inches,Sound Pressure##other##
14 ft Opening TFD 108'' Nozzle,TFD-3-108IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TFD-3-108IG as Specified,111.15625,16.75,21.25,73.75,AGA  ;  Made in USA,14,4000,10600,0.95,200000,320000,28,3,1.5,1725,810,0,30.625,5,>66 dBA
14 ft Opening TFD 120'' Nozzle,TFD-3-120IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TFD-3-120IG as Specified,123.15625,16.75,21.25,73.75,AGA  ;  Made in USA,14,3600,10600,0.94,200000,320000,28,3,1.5,1725,830,0,30.625,5,>66 dBA
14 ft Opening TFD 132'' Nozzle,TFD-3-132IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TFD-3-132IG as Specified,135.15625,16.75,21.25,73.75,AGA  ;  Made in USA,14,3300,10700,0.95,200000,320000,28,3,1.5,1725,1050,0,30.625,5,>66 dBA
14 ft Opening TFD 144'' Nozzle,TFD-4-144IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TFD-4-144IG as Specified,147.21875,16.75,21.25,73.75,AGA  ;  Made in USA,14,4000,14200,0.95,250000,400000,26,4,1.5,1725,1160,0,30.625,5,>66 dBA
14 ft Opening TFD 156'' Nozzle,TFD-4-156IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TFD-4-156IG as Specified,159.21875,16.75,21.25,73.75,AGA  ;  Made in USA,14,3700,14200,0.94,250000,400000,26,4,1.5,1725,1250,0,30.625,5,>66 dBA
14 ft Opening TFD 168'' Nozzle,TFD-4-168IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TFD-4-168IG as Specified,171.21875,16.75,21.25,73.75,AGA  ;  Made in USA,14,3500,14200,0.95,250000,400000,26,4,1.5,1725,1290,0,30.625,5,>66 dBA
17 ft Opening TSD 120'' Nozzle,TSD-2-120IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-2-120IG as Specified,123.125,21,27.25,79.75,AGA  ;  Made in USA,17,3000,9700,0.92,250000,400000,38,2,3,1160,1270,0,30.625,5,>69 dBA
17 ft Opening TSD 132'' Nozzle,TSD-2-132IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-2-132IG as Specified,135.125,21,27.25,79.75,AGA  ;  Made in USA,17,2900,10400,0.863,250000,400000,36,2,3,1160,1290,0,30.625,5,>69 dBA
17 ft Opening TSD 144'' Nozzle 2 Motor,TSD-2-144IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-2-144IG as Specified,147.125,21,27.25,79.75,AGA  ;  Made in USA,17,2900,11200,0.863,250000,400000,33,2,3,1160,1340,0,30.625,5,>69 dBA
17 ft Opening TSD 144'' Nozzle 3 Motor,TSD-3-144IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-144IG as Specified,147.25,21,27.25,79.75,AGA  ;  Made in USA,17,3900,15500,0.951,250000,400000,27,3,3,1160,1560,0,30.625,5,>69 dBA
17 ft Opening TSD 156'' Nozzle,TSD-3-156IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-156IG as Specified,159.25,21,27.25,79.75,AGA  ;  Made in USA,17,3600,15200,0.92,350000,560000,37,3,3,1160,1630,0,48.625,6,>69 dBA
17 ft Opening TSD 168'' Nozzle,TSD-3-168IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-168IG as Specified,171.25,21,27.25,79.75,AGA  ;  Made in USA,17,3500,15900,0.863,350000,560000,35,3,3,1160,1650,0,48.625,6,>69 dBA
17 ft Opening TSD 180'' Nozzle,TSD-3-180IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-180IG as Specified,183.25,21,27.25,79.75,AGA  ;  Made in USA,17,3200,15600,0.863,350000,560000,35,3,3,1160,1690,0,48.625,6,>69 dBA
17 ft Opening TSD 192'' Nozzle 3 Motor,TSD-3-192IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-192IG as Specified,195.25,21,27.25,79.75,AGA  ;  Made in USA,17,3100,16300,0.863,350000,560000,33,3,3,1160,1710,0,48.625,6,>69 dBA
17 ft Opening TSD 204'' Nozzle 3 Motor,TSD-3-204IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-204IG as Specified,207.25,21,27.25,79.75,AGA  ;  Made in USA,17,2900,16000,0.863,400000,640000,37,3,3,1160,1740,0,48.625,6,>69 dBA
17 ft Opening TSD 216'' Nozzle 3 Motor,TSD-3-216IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-3-216IG as Specified,219.25,21,27.25,79.75,AGA  ;  Made in USA,17,2900,16700,0.863,400000,640000,35,3,3,1160,1760,0,48.625,6,>69 dBA
17 ft Opening TSD 192'' Nozzle 4 Motor,TSD-4-192IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-4-192IG as Specified,195.375,21,27.25,79.75,AGA  ;  Made in USA,17,3900,20700,95.1,400000,640000,33,4,3,1160,1930,0,48.625,6,>69 dBA
17 ft Opening TSD 204'' Nozzle 4 Motor,TSD-4-204IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-4-204IG as Specified,207.375,21,27.25,79.75,AGA  ;  Made in USA,17,3600,20400,92,400000,640000,32,4,3,1160,1970,0,48.625,6,>69 dBA
17 ft Opening TSD 216'' Nozzle 4 Motor,TSD-4-216IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - TSD-4-216IG as Specified,219.375,21,27.25,79.75,AGA  ;  Made in USA,17,3600,21100,0.863,400000,640000,31,4,3,1160,2270,0,48.625,6,>69 dBA
22 ft Opening EHD 120'' Nozzle,EHD-2-120IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-2-120IG as Specified,123.125,21,27.25,79.75,AGA  ;  Made in USA,22,4400,15800,0.94,250000,400000,24,2,5,1160,1380,0,30.625,5,>71 dBA
22 ft Opening EHD 132'' Nozzle,EHD-2-132IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-2-132IG as Specified,135.125,21,27.25,79.75,AGA  ;  Made in USA,22,4800,16100,0.95,250000,400000,23,2,5,1160,1600,0,30.625,5,>71 dBA
22 ft Opening EHD 144'' Nozzle,EHD-2-144IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-2-144IG as Specified,147.125,21,27.25,79.75,AGA  ;  Made in USA,22,4800,19200,0.95,250000,400000,19,2,5,1160,1650,0,30.625,5,>71 dBA
22 ft Opening EHD 156'' Nozzle,EHD-3-156IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-3-156IG as Specified,159.25,21,27.25,79.75,AGA  ;  Made in USA,22,4700,20300,0.94,350000,560000,26,3,5,1160,1950,0,48.625,6,>71 dBA
22 ft Opening EHD 168'' Nozzle,EHD-3-168IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-3-168IG as Specified,171.25,21,27.25,79.75,AGA  ;  Made in USA,22,4500,22800,0.94,400000,640000,26,3,5,1160,2010,0,48.625,6,>71 dBA
22 ft Opening EHD 180'' Nozzle,EHD-3-180IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-3-180IG as Specified,183.25,21,27.25,79.75,AGA  ;  Made in USA,22,4400,23000,0.94,400000,640000,26,3,5,1160,2070,0,48.625,6,>71 dBA
22 ft Opening EHD 192'' Nozzle,EHD-3-192IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-3-192IG as Specified,195.25,21,27.25,79.75,AGA  ;  Made in USA,22,4800,23300,0.95,400000,640000,25,3,5,1160,2120,0,48.625,6,>71 dBA
22 ft Opening EHD 204'' Nozzle,EHD-3-204IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-3-204IG as Specified,207.25,21,27.25,79.75,AGA  ;  Made in USA,22,4400,23400,0.94,400000,640000,25,3,5,1160,2230,0,48.625,6,>71 dBA
22 ft Opening EHD 216'' Nozzle,EHD-3-216IG,Powered Aire Indirect Gas Heated Industrial Air Curtain - EHD-3-216IG as Specified,219.25,21,27.25,79.75,AGA  ;  Made in USA,22,4600,24600,0.95,400000,640000,24,3,5,1160,2280,0,48.625,6,>71 dBA
